Specifications



* Low Insertion loss
* Low PDL
* Good channel-to-channel uniformity
* Compact Design
* Wide Operating Wavelength: From 1260nm to 1650nm
* Wide Operating Temperature: From -40°C to 85°C
* High Reliability and Stability
* Applications: FTTX Systems, PON Networks, CATV Links, Optical Signal Distribution
* Compliance: Telcordia GR-1209-CORE, Telcordia GR-1221-CORE, RoHS

 Entry

 Exit

For example:

|  |
| --- |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | Connector type |  | Entry (Number of fibers) |  | Exit (Number of fibers) |  | Fiber type(all cables) |  | Cable lenght in meter(all cables) |
|  |  |   |  |  |  |  |
| **ALWL** |  **-** | **SC** |  **-** | **1** | **X** | **16** |  **-** | **1** |  - | 1 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Available Connector types:** |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Connector:** | SC | SC |   | FC | FC |   | LC | LC |   | ST | ST |   | E2000 | E2000 |
| **Polish:** | APC | UPC |   | APC | UPC |   | APC | UPC |   | APC | UPC |   | APC | UPC |
| **Connector type:** | SCA | SC |   | FCA | FC |   | LCA | LC |   | STA | ST |   | E20 | E2A |

|  |  |
| --- | --- |
| **Available Fiber types:** |   |
|   |   |   |   |
| 1 |  = | OS2 | Singlemode 9/125 |
| 2 |  = | OM1 | Multimode 62,5/125 |
| 3 |  = | OM2 | Multimode 50/125 |
| 4 |  = | OM3 | Multimode 50/125 |
| 5 |  = | OM4 | Multimode 50/125 |

|  |
| --- |
|  |
|  |
|  |  |
|  |
|  |
|  |
|  |