Specifications



* Low Insertion loss
* Low PDL
* Good channel-to-channel uniformity
* Compact Design
* Wide Operating Wavelength: From 1260nm to 1650nm
* Wide Operating Temperature: From -40°C to 85°C
* High Reliability and Stability
* Applications: FTTX Systems, PON Networks, CATV Links, Optical Signal Distribution
* Compliance: Telcordia GR-1209-CORE, Telcordia GR-1221-CORE, RoHS

Entry

Exit

For example:

|  |
| --- |
|  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | Connector type |  | Entry (Number of fibers) |  | Exit (Number of fibers) |  | Fiber type  (all cables) |  | Cable lenght in meter  (all cables) |
|  |  |  |  |  |  |  |
| **ALWL** | **-** | **SC** | **-** | **1** | **X** | **16** | **-** | **1** | - | 1 |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Available Connector types:** | | |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Connector:** | SC | SC |  | FC | FC |  | LC | LC |  | ST | ST |  | E2000 | E2000 |
| **Polish:** | APC | UPC |  | APC | UPC |  | APC | UPC |  | APC | UPC |  | APC | UPC |
| **Connector type:** | SCA | SC |  | FCA | FC |  | LCA | LC |  | STA | ST |  | E20 | E2A |

|  |  |  |  |
| --- | --- | --- | --- |
| **Available Fiber types:** | | |  |
|  |  |  |  |
| 1 | = | OS2 | Singlemode 9/125 |
| 2 | = | OM1 | Multimode 62,5/125 |
| 3 | = | OM2 | Multimode 50/125 |
| 4 | = | OM3 | Multimode 50/125 |
| 5 | = | OM4 | Multimode 50/125 |

|  |
| --- |
|  |
|  |
|  |  |
|  |
|  |
|  |
|  |